#
SUSPENSION

BHE025001013W01

## Suspention

Standard suspension

Item | Specification
--- | ---
Front wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 mm {0.15 in}] | (mm {in}) | 2 {0.08}
Rim inner | (mm {in}) | 1.2±2.5 {0.05±0.09}
Degree | 0°11'±21'
Steering angle [Tolerance ±3°] | Inner | 38°41'
Outer | 33°15'
Steering axis inclination (reference value) | 10°52'
Camber*2 [Tolerance ±1°] | Vehicle height: From the end of the front fender to the center of the wheel (mm {in}) | 367-376 {14.4-14.8} | -0°33'
377-386 {14.9-15.1} | -0°13'
387-396 {15.2-15.5} | 0°04'
397-406 {15.6-15.9} | 0°20'
407-416 {16.0-16.3} | 0°33'
Caster*2 [Tolerance ±1°] | Vehicle height: From the end of the rear fender to the center of the wheel (mm {in}) | 361-370 {14.2-14.5} | 6°31'
371-380 {14.6-14.9} | 6°18'
381-390 {15.0-15.3} | 6°06'
391-400 {15.4-15.7} | 5°53'
401-410 {15.8-16.1} | 5°40'
Rear wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 mm {0.15 in}] | (mm {in}) | 3 {0.12}
Rim inner | (mm {in}) | 1.9±2.5 {0.075±0.098}
| Degree | 0°16'±20'
Camber*2 [Tolerance ±1°] | Vehicle height: From the end of the rear fender to the center of the wheel (mm {in}) | 361-370 {14.2-14.5} | -1°30'
371-380 {14.6-14.9} | -1°12'
381-390 {15.0-15.3} | -0°56'
391-400 {15.4-15.7} | -0°43'
401-410 {15.8-16.1} | -0°33'

  *1 :
Engine coolant and engine oil are at specified level. Jack, and tools are in designated position. Adjust to the median when carrying out wheel alignment.
  *2 :
Difference between left and right must not exceed 1° .

Sport suspension

Item | Specification
--- | ---
Front wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 mm {0.15 in}] | (mm {in}) | 2 {0.08}
Rim inner | (mm {in}) | 1.4±2.8 {0.06±0.11}
| Degree | 0°11'±21'
Steering angle [Tolerance ±3°] | Inner | 38°36'
Outer | 33°07'
Steering axis inclination (reference value) | 11°02'
Camber*2 [Tolerance ±1°] | Vehicle height: From the end of the front fender to the center of the wheel (mm {in}) | 361-370 {14.2-14.5} | -0°45'
371-380 {14.6-14.9} | -0°25'
381-390 {15.0-15.3} | -0°06'
391-400 {15.4-15.7} | 0°11'
401-410 {15.8-16.1} | 0°26'
Caster*2 [Tolerance ±1°] | Vehicle height: From the end of the rear fender to the center of the wheel (mm {in}) | 354-363 {13.9-14.2} | 6°41'
364-373 {14.3-14.6} | 6°28'
374-383 {14.7-15.0} | 6°16'
384-393 {15.1-15.4} | 6°03'
394-403 {15.5-15.8} | 5°50'
Rear wheel alignment (Unloaded)*1 | Total toe-in | Tire [Tolerance ±4 mm {0.15 in}] | (mm {in}) | 3 {0.12}
Rim inner | (mm {in}) | 2.1±2.8 {0.083±0.110}
| Degree | 0°16'±20'
Camber*2 [Tolerance ±1°] | Vehicle height: From the end of the rear fender to the center of the wheel (mm {in}) | 354-363 {13.9-14.2} | -1°44'
364-373 {14.3-14.6} | -1°24'
374-383 {14.7-15.0} | -1°07'
384-393 {15.1-15.4} | -0°52'
394-403 {15.5-15.8} | -0°40'

  *1 :
Engine coolant and engine oil are at specified level. Jack, and tools are in designated position. Adjust to the median when carrying out wheel alignment.
  *2 :
Difference between left and right must not exceed 1° .

Ball joint rotational torque

Item | Specification
--- | ---
Front upper arm ball joint | (N·m {kgf·cm, in·lbf}) | 0.3-2.2 {4-22, 3-19}
Front lower arm ball joint | 0.4-2.9 {5-29, 4-25}
Front stabilizer control link | 0.2-2.0 {3-20, 2-17}
Rear trailing link (upper) | 0.4-3.3 {5-33, 4-29}
Rear lateral link (upper) | 0.4-2.8 {5-28, 4-24}
Rear lateral link (lower) | 0.4-2.8 {5-28, 4-24}
Toe control link | 0.3-2.2 {4-22, 3-19} [Pull scale reading: 3-22 N {0.3-2.2 kgf, 0.7-4.9 lbf}]
Rear stabilizer control link | 0.23-0.47 {2.35-4.79, 2.04-4.15}

## Wheel and Tires

Australian specs.

Item | Specification
--- | ---
Standard tire wheel | Size | 16 x 7 1/2JJ | 18 x 8JJ
Offset | (mm {in}) | 50 {2.0}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Aluminum alloy
Standard tire | Size | 225/55R16 95V | 225/45R18 91W
Air pressure | (kPa {kgf/cm2, psi}) | 220 {2.2, 32}
Remaining tread | (mm {in}) | 1.6 {0.063} min.
Standard tire wheel and tire | Lug nut tightening torque | (N·m {kgf·m, ft·lbf}) | 89-117 {9.0-12.0, 65.0-87.0}
Wheel and tire runout | Radial direction | 1.5 {0.059} max.
(mm {in}) | Lateral direction | 2.0 {0.078} max.
Wheel imbalance | (g {oz}) | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.

  *1 :
Total weight exceeds 160 g {5.65 oz}.
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.

European (L.H.D. U.K.) specs..

Item | Specification
--- | ---
Standard tire wheel | Size | 16 x 7 1/2JJ | 18 x 8JJ
Offset | (mm {in}) | 50 {2.0}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Material | Aluminum alloy
Standard tire | Size | 225/55R16 95V | 225/45R18 91W
Air pressure (kPa {kgf/cm2, psi}) | Front | 4 persons or less | 220 {2.2, 32}
Full load | 220 {2.2, 32}
Rear | 4 persons or less | 220 {2.2, 32}
Full load | 250 {2.6, 36} | 270 {2.8, 39}
Remaining tread | (mm {in}) | 1.6 {0.063} min.
Standard tire wheel and tire | Lug nut tightening torque | (N·m {kgf·m, ft·lbf}) | 89-117 {9.0-12.0, 65.0-87.0}
Wheel and tire runout | Radial direction | 1.5 {0.059} max.
(mm {in}) | Lateral direction | 2.0 {0.078} max.
Wheel imbalance | (g {oz}) | Adhesive-type*1: 13 {0.46} max. Knock-type*2: 8 {0.28} max. | Adhesive-type*1: 10 {0.35} max. Knock-type*2: 6 {0.21} max.

  *1 :
Total weight exceeds 160 g {5.65 oz}.
  *2 :
One balance weight: 60 g {2.12 oz} max. If the total weight exceeds 100 g {3.53 oz} on one side, rebalance after moving the tire around on the rim. Do not use three or more balance weights.