#
TOE CONTROL LINK INSPECTION

BHE021428451W02

1. Remove the toe control link from the vehicle.

2. Inspect the lateral link for bending or damage. If there is any malfunction, replace the lateral link.

3. Inspect the ball joint for looseness. If there is any malfunction, replace the ball joint.

4. Rotate the ball joint 5 times.

5. Install the SST to the ball stud, and measure the ball joint rotational torque using a pull scale.

  Toe control link ball joint rotational torque
  0.3-2.2 N·m {4-22 kgf·cm, 3-19 in·lbf}
  Pull scale reading: 3-22 N {0.3-2.2 kgf, 0.7-4.9 lbf}

  • If not within the specification, replace the toe control link.