#
REAR DRIVE SHAFT INSPECTION

BHE031325600W02

1. Verify that the drive shaft is not twisted or damaged.

  • If there is any malfunction, replace the applicable part.

2. Inspect the dust boot for damage and cracks.

  • If there is any malfunction, replace the applicable part.

3. Move the spline and joint up and down, left and right by hand and verify that there is no roughness.

  • If there is any malfunction, replace the applicable part.