#
THERMOSTAT INSPECTION

BHE011215171W02

1. Inspect the thermostat for the following.

  Warning

  • During inspection, the thermostat and water are extremely hot and they can cause burns. Do not touch the thermostat and water.

  • The valve shall not open under normal temperature.
  • Opening temperature and valve lift

  – If there is any malfunction, replace the thermostat.

Item | Specification
--- | ---
Initial-opening temperature | (°C {°F}) | 80-84 {176-183}
Full-open temperature | (°C {°F}) | 95 {203}
Full-open lift | (mm {in}) | 8.5 {0.33} or more