#
DRIVE BELT CONSTRUCTION

BHE011015800T01

• The V-ribbed drive belts are composed of two belts, one that drives the generator and the water pump, and another that drives the A/C compressor. Serviceability has been improved from this simple layout based on the motorization of the air pump and P/S pump that were formerly driven by drive belts.

1 | Generator pulley
2 | Drive belt
3 | Water pump pulley
4 | Eccentric shaft pulley
5 | Tensioner pulley
6 | A/C compressor pulley