#
FRONT TILT MOTOR INSPECTION

BHE091388650W01

1. Disconnect the front tilt motor connector.

2. Connect battery positive voltage to front tilt motor terminal A or B, then verify that the front tilt motor operate as shown in the table.

  • If the front tilt motor does not operate as indicated in the table, replace the front tilt motor.

Motor operation | Connection
--- | ---
B+ | GND
Up | B | A
Down | A | B