#
REAR DOOR REMOVAL/INSTALLATION

BHE091158010W03

1. Disconnect the negative battery cable.

2. Remove the rear seat cushion. (See REAR SEAT REMOVAL/INSTALLATION.)

3. Remove the seat belt rail. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

4. To remove the checker, remove the following parts:

  (1) Rear door lower trim (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

5. To remove the rear door hinge, remove the following parts:

  (1) Rear seat cushion (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

1 | Connector
2 | Bolt A
3 | Bolt B
4 | Rear door
5 | Bolt C
6 | Checker
7 | Nut
8 | Rear door hinge

7. Install in the reverse order of removal.

8. Adjust the rear door. (See DOOR ADJUSTMENT.)