#
AUDIO AMPLIFIER REMOVAL/INSTALLATION

BHE092066910W01

## Main Amplifier

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Console (See CONSOLE REMOVAL/INSTALLATION.)
  (2) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (5) Rear package center trim, rear package side trim (See REAR PACKAGE TRIM REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Bolt
2 | Connector
3 | Main amplifier

4. Install in the reverse order of removal.

## Front Door Speaker Amplifier

1. Disconnect the negative battery cable.

2. Remove the front door trim. (See FRONT DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the front door speaker. (See FRONT DOOR SPEAKER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Bolt
2 | Front door speaker amplifier

5. Install in the reverse order of removal.