#
POWER OUTER MIRROR SWITCH REMOVAL/INSTALLATION

BHE091266600W01

1. Disconnect the negative battery cable.

2. Disengage clips using a tape-wrapped flathead screwdriver.

3. Remove the switch panel from the front door trim keeping the tab from catching.

4. Disconnect the power window main switch connector and power outer mirror switch connector.

5. Remove the screws and the power outer mirror switch.

6. Install in the reverse order of removal.