#
TRANSMISSION OIL INSPECTION [Y16M-D]

BHE051127001W03

1. Position the vehicle on level ground.

2. Remove oil filler plug.

3. Verify that the oil is near the brim of the plug port.

  • If the oil is not near the brim of the plug port, add the specified amount and type of oil.

  Specified oil grade
  API Service GL-4 or GL-5
  Specified oil viscosity
  SAE 75W-90

4. Install oil filler plug and a new washer.

  Tightening torque
  27-48 N·m {2.8-4.9 kgf·m, 20-35 ft·lbf}