#
TRUNK LID LATCH AND OPENER REMOVAL/INSTALLATION

BHE091467005W01

1. Disconnect the negative battery cable.

2. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Detach the rod.

4. Disconnect the trunk lid opener connector and the trunk compartment light connector.

5. Remove the bolts, then remove the trunk lid latch and opener.

6. Install in the reverse order of removal.