#
REVERSE LOCKOUT MECHANISM CONSTRUCTION/OPERATION [R15M-D]

BHE051117570T02

• A cam-type reverse lockout mechanism is adopted to ensure reliability.

• A cam, which is installed to the shift guide plate in the shift control case, restricts the selector movement to prevent the driver from misshifting.

• When shifting into reverse, by shifting the selector back into the neutral position once and then shifting to the 5th/reverse direction, the selector pushes the cam outward to release the shifting restriction, and shifting into reverse is made possible.

Shift guide component operation

1 | Shifting directly from 5th into reverse
2 | Shifting into reverse after shifting into neutral
3 | Restricts movement
4 | Restriction released
5 | Selector
6 | 4th
7 | 3rd
8 | Reverse
9 | 5th
10 | Neutral