#
PARAMETER IDENTIFICATION (PID) DATA MONITORING FUNCTION

BHE050201026T07

• The PID mode allows access to certain data values, analog and digital input and output, calculations and system state information.

## Monitor Item Table

Display on the tester | Definition | Unit/Condition | TCM terminal
--- | --- | --- | ---
24B_Duty | Shift solenoid valve B (2-4 brake duty) | % | 2S
BOO_TCM | Brake switch | ON/OFF | 1G
CPP/PNP | TR switch (P/N position switch) | Drive/Neutral | 1D, 2B
DTC_CNT | Number of DTCs detected | N/A | N/A
DWN SW | Down switch (manual mode) | ON/OFF | 2D
ECT TCM | Engine coolant temperature | °C, °F | N/A
FDPDTC | Pending code causing FFD storage | N/A | N/A
GEAR | Calculated gear ratio in TCM | 1st/2nd/3rd/4th | N/A
GEAR_RA | Calculated gear ratio in TCM | N/A | N/A
HC_Duty | Shift solenoid valve C (high clutch duty) | % | 2V
LRB_Duty | Shift solenoid valve F (low and reverse brake duty) | % | 2P
LU_Duty | TCC solenoid valve (TCC solenoid duty) | % | 2W
MNL SW | M range switch | ON/OFF | 1E
OP_SW_24B | Oil pressure switch B | ON/OFF | 2A
OP_SW_HC | Oil pressure switch C | ON/OFF | 2F
OP_SW_LRB | Oil pressure switch F | ON/OFF | 2H
OSS | Vehicle speed sensor (output shaft speed signal) | rpm | 2K
PCSV | Pressure control solenoid valve | ON/OFF | 2X
RPM | Engine speed | rpm | N/A
TCCC | Shift solenoid valve A (low clutch duty) | % | 2Y
TFT | ATF temperature | °C, °F | 2J
TFTV | ATF temperature signal voltage | V | 2J
THOP | Throttle position | % | N/A
TR | TR switch | R/N/D | 2B, 2C, 2E
TRD | TR switch (D range switch) | ON/OFF | 2E
TRR | TR switch (R position switch) | ON/OFF | 2C
TSS | Turbine sensor | rpm | 2G
UP SW | Up switch (manual mode) | ON/OFF | 2I
VPWR | Battery voltage | V | 1A, 2Z, 2AA
VSS | Vehicle speed | km/h, mph | N/A