#
POWER SEAT SWITCH INSPECTION

BHE091357155W01

## Power Seat Switch

1. Disconnect the power seat switch connector.

2. Verify that the continuity between the power seat switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the power seat switch.

## Lumbar Support Switch

1. Disconnect the lumbar support switch connector.

2. Verify that the continuity between the lumbar support switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the lumbar support switch.