#
CLUTCH COVER INSPECTION

BHE051016410W01

1. Remove the clutch cover.

2. Measure the wear of the diaphragm spring fingers using a vernier caliper.

  Maximum wear
  0.6 mm {0.024 in}

  • If it exceeds the maximum specification, replace the clutch cover.

3. Measure the pressure plate flatness using a straight edge and a feeler gauge.

  Note

  • Measure the pressure plate flatness across the center.

  Maximum flatness
  0.5 mm {0.020 in}

  • If it exceeds the maximum specification, replace the clutch cover.

4. Attach a dial gauge to the rear housing, rotate the flywheel, then inspect for height difference between the diaphragm spring fingers.

  Maximum height difference
  1.0 mm {0.039 in}

  • If it exceeds the maximum specification, replace the clutch cover.