#
SEQUENTIAL DYNAMIC AIR INTAKE SYSTEM (S-DAIS) STRUCTURE

BHE011300113T06

• The S-DAIS is composed of the SSV, VDI valve, and VFAD valve (13B-MSP (High Power)) which are opened and closed by intake manifold vacuum or BARO, and the APV (13B-MSP (High Power)) which is opened and closed by motor drive.

1 | Illustration shows 13B-MSP (High power)
2 | APV motor (13B-MSP (High power))
3 | SSV actuator
4 | SSV
5 | VDI valve
6 | VDI actuator
7 | Intake manifold
8 | APV (13B-MSP (High power))
9 | Check valve
10 | Vacuum chamber
11 | SSV solenoid valve
12 | VDI solenoid valve
13 | VFAD solenoid valve(13B-MSP (High power))
14 | Extension manifold
15 | Check valve (13B-MSP (High power))
16 | Vacuum chamber(13B-MSP (High power))
17 | VFAD actuator (13B-MSP (High power))
18 | VFAD valve (13B-MSP (High power))