#
HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION

BHE091966122W10

1. Disconnect the negative battery cable.

2. Remove the front side turn light. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Disconnect joint pipe.

5. Disconnect headlight cleaner hose from the headlight cleaner actuator.

6. Remove the headlight cleaner hose from the front bumper.

7. Install in the reverse order of removal.