#
REAR DOOR UPPER TRIM REMOVAL/INSTALLATION

BHE091768400W02

1. Remove the upper anchor of the front seat belt. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

2. Remove the rear door lower trim. (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

3. Pull the rear door upper trim outward and detach clips A, B and locator pins C from the body.

4. Remove the rear door upper trim.

5. Install in the reverse order of removal.