#
PASSENGER AIR BAG DEACTIVATION (PAD) SWITCH INSPECTION

BHE081066123W05

1. Remove the hole cover. (R.H.D.) (See CONSOLE REMOVAL/INSTALLATION.)

2. Remove the PAD switch. (See PASSENGER AIR BAG DEACTIVATION (PAD) SWITCH REMOVAL/INSTALLATION.)

3. Verify that the continuity between the PAD switch terminals is as indicated in the table.

  • If not as indicated in the table, replace the PAD switch.