#
REAR PILLAR TRIM REMOVAL/INSTALLATION

BHE091768150W01

1. Remove the rear seat. (See REAR SEAT REMOVAL/INSTALLATION.)

2. Remove the inner scuff plate. (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)

3. Remove the tire house trim. (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)

4. Remove the cap using a fastener remover. (Vehicles with curtain air bags)

5. Remove the bolt. (Vehicles with curtain air bags)

6. Remove the fastener.

7. Detach clips A and locator pin B, using a fastener remover, and remove the rear pillar trim.

8. Install in the reverse order of removal.