#
DLC-2 CONSTRUCTION

BHE040243000T06

• A connector (DLC-2) conforming to International Organization for Standardization (ISO) standards has been added.

• Shape and terminal arrangement as stipulated by the ISO 15031-3 (SAE J1962) international standard has been adopted for this connector. The connector has a 16-pin construction that includes the KLN, CAN_H, CAN_L, GND1, GND2 and B+ terminals.

Terminal | Function
--- | ---
KLN | Serial communication terminal (malfunction diagnosis use)
CAN_L | Serial communication terminal (Lo)
CAN_H | Serial communication terminal (Hi)
GND1 | Body ground terminal
GND2 | Serial communication ground terminal
B+ | Battery power supply terminal