#
REAR DOOR GLASS REMOVAL/INSTALLATION

BHE091259500W02

1. Remove the inner handle cover.

2. Remove the rear door lower trim. (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

3. Remove the rear door upper trim. (See REAR DOOR UPPER TRIM REMOVAL/INSTALLATION.)

4. Pull up the rear door weatherstrip and remove the screw.

5. Remove the bolts.

6. Remove the rear door glass.

7. Install in the reverse order of removal.