#
FRONT LOWER ARM REMOVAL/INSTALLATION

BHE021334300W01

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled while servicing the vehicle.

1. Remove the front suspension tower bar. (See FRONT SUSPENSION TOWER BAR REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Caliper and mounting support (See Caliper and Mounting Support Removal Note.)
2 | Disc plate
3 | Tie-rod end (See Tie-rod End Removal Note.)
4 | Front lower arm boll joint (See Front Lower Arm Ball Joint Removal Note.)
5 | Front upper arm ball joint (See Upper Arm Ball Joint Removal Note.)
6 | Stabilizer control link nut (front lower arm side)
7 | Shock absorber and front upper arm
8 | Front lower arm
9 | Clip (See Clip Installation Note.)
10 | Dust boot
11 | Bushing (rear side) (See Bushing (Rear Side) Removal Note.) (See Bushing (Rear Side) Installation Note.)
12 | Bushing (front side) (See Bushing (Front Side) Removal Note.) (See Bushing (Front Side) Installation Note.)
13 | Bushing (shock absorber lower side connecting part) (See Bushing (Shock Absorber Lower Side Connecting Part) Removal Note.) (See Bushing (Shock Absorber Lower Side Connecting Part) Installation Note.)

## Caliper and Mounting Support Removal Note

1. Remove the caliper and mounting support from the steering knuckle and suspend it with a cable in a location out of the way.

## Front Lower Arm Ball Joint Removal Note

1. Disconnect the front lower arm ball joint from the steering knuckle using the SST.

  Note

  • When removing the front lower arm ball joint, the steering knuckle bushing may also come off. If it comes off, replace the steering knuckle.

## Upper Arm Ball Joint Removal Note

1. Loosen the bolts on the vehicle side.

2. Disconnect the upper arm ball joint using the SST.

## Bushing (Rear Side) Removal Note

1. Mark the front upper arm as shown in the figure.

2. Remove the bushing using the SSTs.

## Bushing (Front Side) Removal Note

1. Cut off the stopper plate rubber using a razor.

2. Cut off 5-6 mm {0.20-0.23 in} from each side of the knob end of the bushing using a hacksaw.

## Bushing (Shock Absorber Lower Side Connecting Part) Removal Note

1. Remove the bushing using the SSTs.

## Bushing (Shock Absorber Lower Side Connecting Part) Installation Note

1. Compress the bushing using the SSTs.

## Bushing (Front Side) Installation Note

1. Press the bushing in using the SSTs.

2. Insert the stopper plate rubber into the inner pipe of the bushing (front side).

## Bushing (Rear Side) Installation Note

1. Align the marks placed during removal and install the bushing.

2. Press the bushing in using the SSTs.

## Clip Installation Note

1. Wipe the grease off the ball joint stud.

2. Fill the inside of the new dust boot with grease.

3. Install the dust boot to the ball joint.

4. Install the clip using the SST.

5. Verify that the clip is installed securely to the groove.

6. Wipe off any excess grease.