#
SUSPENSION SPECIFICATIONS

BHE020001013T03

Suspension

Item | Specification
--- | ---
Standard suspension | Sport suspension
Front suspension | Type | Double-wishbone
Spring type | Coil spring
Shock absorber type | Monotube type: High-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 25.4 {1.00} | 26.5 {1.04}
Wheel alignment (Unloaded*) | Total toe-in | Tire [Tolerance ±4 {0.15}] | (mm {in}) | 2 {0.08}
Rim inner | 1.2±2.5 {0.05±0.09} | 1.4±2.8 {0.06±0.11}
Degree | 0°11'±21'
Maximum steering angle [Tolerance ±3°] | Inner | 38°41' | 38°36'
Outer | 33°15' | 33°07'
Caster angle (Reference) [Tolerance ±45'] | 6°06' | 6°15'
Camber angle (Reference) [Tolerance ±45'] | 0°04' | -0°06'
Steering axis inclination (Reference) | 10°52' | 11°02'
Rear suspension | Type | Multi-link
Spring type | Coil spring
Shock absorber type | Monotube type: High-pressure gas charged, cylindrical, double-acting
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 15.9 {0.626}
Wheel alignment (Unloaded*) | Total toe-in | Tire [Tolerance ±4 {0.15}] | (mm {in}) | 3 {0.12}
Rim inner | 1.9±2.5 {0.075±0.098} | 2.1±2.8 {0.083±0.110}
Degree | 0°16'±20'
Camber angle [Tolerance ±45'] | -0°56' | -1°07'

  * :
Unloaded: Fuel tank is full. Engine coolant and engine oil are at specified level. Jack and tools are in designated position.

Wheel and Tire

Item | Specification
--- | ---
Tire | Size | 225/55R16 95V | 225/45R18 91W
Wheel | Size | 16 x 7 1/2JJ | 18 x 8JJ
Material | Aluminum alloy
Offset | (mm {in}) | 50 {2.0}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}