#
MAIN FUSE REMOVAL/INSTALLATION

BHE092166761W01

1. Disconnect the negative battery cable.

2. Remove the main fuse block cover.

3. Remove in the order indicated in the table.

1 | Connector
2 | Nut
3 | Bolt (See Bolt Removal Note.)
4 | Main fuse

4. Install in the reverse order of removal.

## Bolt Removal Note

1. Press the tabs in the direction indicated by the arrows, lift the main fuse block, and then remove the bolt.