#
SELECTOR LEVER OUTLINE

BHE051446010T01

• Operability has been improved due to the short stroke feature of the selector lever.

• Shift position has been optimized by the reduction of space achieved between the frequently utilized N and D ranges. Due to this optimization of shift position, a quick and sporty shift operation has been achieved while the sleek shift feeling of an AT is also maintained.