#
BONNET REMOVAL/INSTALLATION

BHE091056601W01

  Warning

  • Removing the bonnet without proper support can be dangerous. The bonnet may fall and injure you. Always perform the following procedure with at least another person.

1. Disconnect the negative battery cable.

2. To remove the bonnet hinge, remove the following parts:

  (1) Front side turn lights (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)
  (2) Front bumper (See FRONT BUMPER REMOVAL/INSTALLATION.)
  (3) Front combination lights (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)
  (4) Front fender panel (See FRONT FENDER PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Bonnet insulator
2 | Shroud seal weatherstrip
3 | Bonnet
4 | Bonnet hinge
5 | Bonnet stay

4. Install in the reverse order of removal.

5. Adjust the bonnet. (See BONNET ADJUSTMENT.)