#
EVAPORATOR TEMPERATURE SENSOR REMOVAL/INSTALLATION

BHE074061022W01

1. Disconnect the negative battery cable.

2. Remove the glove compartment. (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove the keyless unit. (See KEYLESS UNIT REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Evaporator temperature sensor connector
2 | Evaporator temperature sensor

5. Install in the reverse order of removal.