#
TURBINE SENSOR CONSTRUCTION/OPERATION

BHE051319200T06

• The turbine sensor is a Hall element type. A 32-pulse signal is generated per rotation of the reverse and high clutch drum and the sensor sends this signal to the TCM.

• The TCM detects the shift start and end timing according to the signal from turbine sensor, and performs detailed control, improving shift quality.

1 | Turbine sensor
2 | Reverse and high clutch drum
3 | Power supply
4 | Output
5 | Ground
6 | Input wave form