#
DTC 22

BHE070201038W16

DTC 22 | Airflow mode actuator (potentiometer) system inspection
--- | ---
POSSIBLE CAUSE | • Airflow mode actuator malfunction • Open circuit in wiring harness between A/C amplifier and airflow mode actuator • Short circuit in wiring harness between A/C amplifier (terminal 2G) and air mix actuator (terminal E)

Diagnostic Procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect the airflow mode actuator. (See AIRFLOW MODE ACTUATOR INSPECTION.) • Is it normal? | Yes | Go to the next step.
No | Replace the airflow mode actuator. (See AIRFLOW MODE ACTUATOR REMOVAL/INSTALLATION.)
2 | • Disconnect the A/C amplifier connector (16-pin) and the airflow mode actuator connector. • Is there an open circuit in the wiring harness between the following terminals of the A/C amplifier connector (16-pin) and the airflow mode actuator connector? – 2O-A – 2G-E – 2P-C | Yes | Repair the wiring harness.
No | Go to the next step.
3 | • Is there a short circuit to ground in the wiring harness between A/C amplifier connector (16-pin) terminal 2G and airflow mode actuator connector terminal E? | Yes | Repair the wiring harness.
No | The system is normal at present. (Clear the past malfunction from memory.)