#
IGNITION COIL INSPECTION

BHE011801009W03

## Ignition Coil With Built-in Power Switch Inspection

1. Disconnect the ignition coil connector.

2. Measure the resistance between each terminal on the ignition coil connector.

  • If the measurement corresponds to the table, replace the ignition coil.

Item | Tester Connection Position | Condition
--- | --- | ---
Positive | Negative
Terminal | A | B | ∞ or 0 ohm is abnormal
B | C
C | A | 0 to several kilohm (continuity) is abnormal