#
COMBINED SENSOR CONSTRUCTION/OPERATION

BHE041543770T02

• The combined sensor, with built-in yaw rate and lateral-G sensors, detects and calculates the vehicle yaw rate and lateral-G, converts them into voltage and transmits this to the DSC HU/CM.

• The output voltage characteristic for the combined sensor is 2.5 V when the vehicle is standing still, and changes accordingly as yaw rate and lateral-G are formed.

• The yaw rate sensor detects a Coriolis force created by, and in proportion to, the rotation speed of a rotating tuning fork.

• The lateral-G sensor detects an inertial force created by, and in proportion to, a G-force acting on a silicon detection component.

  Note

  • Coriolis force: When an object on a rotating disc attempts to move toward the center of the disc, force is produced at a right angle to the intended path of travel of the object. This results in the direction of movement being unchanged from its original point of departure, and the object does not reach the center. When looking at this effect from outside the disc, it appears as if a force is deflecting the object away from the center. This appearance of force is called a Coriolis force, and the object actually advances in a straight course.

1 | Structural view
2 | Vehicle front