#
STATIONARY GEAR CONSTRUCTION

BHE011010908T06

• The special steel used for the stationary gear is processed with ion nitriding for improved strengthening against fatigue on the tooth surfaces.

• The main bearing is pressed into the stationary gear. Rotation lock of this bearing is done with a screw for the high power and a rotation lock tab for the standard power.

• A needle bearing and thrust plate have been assembled in the front stationary gear for regulation of the eccentric shaft end play.

1 | Stationary gear (standard power)
2 | Main bearing
3 | Front stationary gear
4 | Rear stationary gear
5 | Rotation lock tab
6 | Plate
7 | Needle bearing
8 | Thrust plate
9 | Screw (high power)