#
PLASTIC PARTS HEAT RESISTING TEMPERATURE

BHE098050000B01

Part Name | Code | Material Name | Heat resisting Temperature°C {°F}
--- | --- | --- | ---
WINDSHIELD MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
COWL GRILLE | PP | POLYPROPYLENE | 100 {212}
FRONT COMBINATION LIGHT | LENS | PC | POLYCARBONATE | 130 {266}
HOUSING | PP | POLYPROPYLENE | 95 {203}
FRONT BUMPER | PP | POLYPROPYLENE | 100 {212}
FRONT SIDE MARKER LIGHT | LENS | PMMA | ACRYLIC | 75 {167}
HOUSING | ASS | ASS | 80 {176}
OUTER HANDLE | HANDLE BASE | PC-PET | POLYCARBONATE-PET | 80 {176}
HANDLE LEVER | PC-PBT | POLYCARBONATE-PBT | 80 {176}
OUTSIDE MIRROR | ABS | ABS | 90 {194}
REAR COMBINATION LIGHT | LENS | PMMA | ACRYLIC | 80 {176}
HOUSING | AES | AES | 70 {158}
REAR BUMPER | PP | POLYPROPYLENE | 100 {212}
HIGH-MOUNT BRAKE LIGHT | PC | POLYCARBONATE | 100 {212}
ROOF MOULDING | PVC | POLYVINYLCHLORIDE | 95 {203}
BELTLINE MOLDING | PVC | POLYVINYLCHLORIDE | 95 {203}
FENDER GRILLE | PP | POLYPROPYLENE | 100 {212}
REAR SPOILER | SMC | SEAT MOLDING COMPOUND | 90 {194}

  Note

  • The application of temperatures higher than heat resisting temperatures may result in part deformation.