#
REAR PACKAGE TRIM REMOVAL/INSTALLATION

BHE091768300W01

1. Remove the following parts:

  (1) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (2) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (3) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (4) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)

2. Remove the rear package side trim fasteners.

3. Pull the rear package side trim upward and detach clips A from the body.

4. Detach tabs B and pin C from the rear package center trim.

5. Detach tabs D from the body and remove the rear package side trim.

6. Pull the rear package center trim upward and detach clips A, tabs E, and locator pin F from the body.

7. Detach tabs D from the body and remove the rear package center trim.

8. Install in the reverse order of removal.