#
REAR DOOR RELEASE HANDLE REMOVAL/INSTALLATION

BHE091459320W02

1. Remove the rear door lower trim. (See REAR DOOR LOWER TRIM REMOVAL/INSTALLATION.)

2. Remove the rear door upper trim. (See REAR DOOR UPPER TRIM REMOVAL/INSTALLATION.)

3. Remove the bolts, then remove the rear door release handle.

4. Detach the rear door upper and lower latch cables.

5. Install in the reverse order of removal.