#
SIDE SILL PANEL FRONT INSTALLATION

BHE098070270B02

1. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension, then adjust the position to align it to the standard dimensions.

  Caution

  • When cutting and joining the side sill reinforcement, make sure not to damage or scratch the side sill gusset.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.