#
INTRUDER SENSOR REMOVAL/INSTALLATION

BHE091400172W01

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)
  (2) Sunroof seaming welt (vehicles with sunroof)
  (3) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)
  (4) Rear seat (See REAR SEAT REMOVAL/INSTALLATION.)
  (5) Inner scuff plate (See INNER SCUFF PLATE REMOVAL/INSTALLATION.)
  (6) Tire house trim (See TIRE HOUSE TRIM REMOVAL/INSTALLATION.)
  (7) Rear pillar trim (See REAR PILLAR TRIM REMOVAL/INSTALLATION.)
  (8) Map light (See MAP LIGHT REMOVAL/INSTALLATION.)
  (9) Interior light (See INTERIOR LIGHT REMOVAL/INSTALLATION.)
  (10) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)
  (11) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

3. Disconnect the keyless unit connector.

4. Remove the bolts.

5. Remove the intruder sensor.

6. Install in the reverse order of removal.