#
TORQUE CONVERTER CLUTCH (TCC) CONTROL STRUCTURE

BHE051318901T16

## Features

• The TCM selects the TCC schedule according to the gear selected by the transmission. Fifty Hz (20 ms cycle) on/off signals are relayed from the TCC schedule, VSS and throttle opening angle to the duty cycle TCC solenoid valve to control the TCC.

## Structure

System diagram

1 | Turbine sensor
2 | Throttle opening signal
3 | Engine peed signal
4 | TFT sensor
5 | M range switch
6 | TCC solenoid