#
ECCENTRIC SHAFT POSITION PLATE REMOVAL/INSTALLATION

BHE014011430W02

1. Remove the drive belt referring to the drive belt replacement. (See DRIVE BELT REPLACEMENT.)

  Caution

  • To allow the PCM to identify that the eccentric shaft position plate has been replaced, pump the brake pedal 20 times within 8 s after the ignition switch is turned to the ON position (engine off).

2. Remove in the order indicated in the table.

.

1 | Drive belt pulley
2 | Eccentric shaft position plate

3. Install in the reverse order of removal.