#
TARGET TEMPERATURE OPERATION

BHE074061190T03

## Target Temperature Calculation

• The target temperature is calculated using the following formula based on input from the cabin temperature sensor, the ambient temperature sensor and the solar radiation sensor, in addition to the temperature set by the climate control unit.

  Target temperature = (K1 x set temperature) - (K2 x cabin temperature) - (K3 x ambient temperature) - (K4 x solar radiation temperature) + K5 + C
  K1-K5 :
Control coefficient
  C :
Correction coefficient