#
OIL NOZZLE REMOVAL/INSTALLATION

BHE011114100W02

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.

1. Remove the engine cover. (See ENGINE COVER REMOVAL/INSTALLATION.)

2. Remove the battery cover.

3. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION.)

4. Remove the battery, battery box, and battery tray. (See BATTERY REMOVAL/INSTALLATION.)

5. Remove extension manifold. (upper, lower) (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

8. Start the engine and confirm that there is no oil leakage from areas worked on.

  • If there is any oil leakage, find the cause and repair or replace the applicable part.

9. Inspect the oil level. (See ENGINE OIL LEVEL INSPECTION.)

1 | Air hose
2 | Oil nozzle
3 | Washer
4 | Oil pipe (housing side)
5 | Washer