#
REAR SPEAKER INSPECTION

BHE092066961W04

1. Verify the resistance between rear speaker terminals.

  • If the resistance is not within the specification, replace the rear speaker.

  Resistance
  Standard: 4 ohms
  BOSE: 2 ohms

2. Connect a 1.5 V battery to the rear door speaker and verify that noise is sound from the rear door speaker.

  • If no sound is output, replace the rear door speaker.