#
FRONT SIDE FRAME OUTER INSTALLATION

BHE098053300B04

1. When installing new parts, position each part so that the section measurement aligns with the body dimension.

2. Drill holes for plug welds before installing new parts.

3. Weld the one locations indicated by (A), then temporarily installing the inner and outer.

4. After temporarily installing new parts, make sure the related parts fit properly.