#
FRONT FOG LIGHT REMOVAL/INSTALLATION

BHE091851680W01

## LH

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Disconnect the connector.

5. Remove the screws, then remove the front fog light.

6. Install in the reverse order of removal.

7. Adjust the front fog light aiming. (See FRONT FOG LIGHT AIMING.)

## RH

1. Disconnect the negative battery cable.

2. Remove the front side turn lights. (See FRONT SIDE TURN LIGHT REMOVAL/INSTALLATION.)

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Disconnect the connector.

5. Remove screws A and pull back the front fog light cover in the direction of the arrow.

6. Remove screw B, then remove the front fog light cover.

7. Remove screws C, then remove the front fog light.

8. Install in the reverse order of removal.

9. Adjust the front fog light aiming. (See FRONT FOG LIGHT AIMING.)