#
BRAKES

BHE045001020W01

Item | Specification
--- | ---
CONVENTIONAL BRAKE SYSTEM
Brake pedal | Pedal height (reference value) | (mm {in}) | 175 {6.89}
Pedal play | (mm {in}) | 2-5 {0.08-0.19}
Pedal-to-floor clearance (Brake pedal when depressed at 147 N {15.0 kgf, 33 lbf}) | (mm {in}) | 98.6 {3.88} or more
Power brake unit | Fluid pressure when pedal depressed at 200 N {20.4 kgf, 44.9 lbf} | At 0 kPa {0 mmHg, 0 inHg} | 606 {6.18, 87.9} or more
(kPa {kgf/cm2, psi}) | At 66.7 kPa {500 mmHg, 19.7 inHg} | 7,310 {74.54, 1,060} or more
Front brake (disc) | Minimum disc pad thickness | (mm {in}) | 2.0 {0.079}
Minimum disc plate thickness | (mm {in}) | 22 {0.87}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Rear brake (disc) | Minimum disc pad thickness | (mm {in}) | 2.0 {0.079}
Minimum disc plate thickness | (mm {in}) | 16 {0.63}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Brake fluid | Type | European (L.H.D. U.K.) specs.: SAE J1703, FMVSS 116 DOT3 or DOT4 Australian specs.: SAE J1703, FMVSS 116 DOT3
PARKING BRAKE SYSTEM
Parking brake lever | Lever stroke when pulled with 98 N {10 kgf, 22 lbf} at point 50 mm {1.97 in} from the end of the parking brake lever | (notches) | 1-3