#
REAR BUMPER REMOVAL/INSTALLATION

BHE091050210W01

1. Disconnect the negative battery cable.

2. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

3. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

4. Remove the rear combination lights. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

5. Remove the fasteners.

6. Pull the rear bumper guard outward, detach tabs A, and then remove the rear bumper guard.

7. Remove in the order indicated in the table.

1 | Fastener A
2 | Screw A
3 | Fastener B
4 | Fastener C
5 | Screw B
6 | Rear bumper (See Rear Bumper Removal Note.) (See Rear bumper Installation Note.)

8. Install in the reverse order of removal.

## Rear Bumper Removal Note

1. Pull the rear bumper ends (wheel arch) outward to detach from the bumper slider.

  Caution

  • When detaching the rear bumper from the bumper slider, the rear bumper could fall and be damaged. Secure the rear bumper so that it does not fall.

## Rear bumper Installation Note

1. Spread the rear bumper ends (wheel arches) apart.

2. Attach the rear bumper to the body.

3. Press the rear bumper connecting area into the body to engage with the bumper slider.