#
REFRIGERANT LINES CONSTRUCTION

BHE071161460T01

• Aluminum alloy has been adopted for the pipes of the refrigerant lines and rubber (flexible hoses) has been adopted for the hoses.

• A high-pressure charging valve is installed on cooler pipe No.2, and a low-pressure charging valve is installed on the cooler hose (LO).

1 | Cooler pipe No.1
2 | Cooler pipe No.2
3 | Cooler hose (LO)
4 | Cooler hose (HI)
5 | Low-pressure charging valve
6 | High-pressure charging valve