#
SUNROOF UNIT CONSTRUCTION/OPERATION

BHE091569850T01

• Consists of a glass panel, frame and sunroof motor.

• The drive cables inside the frame are engaged with the sunroof motor drive gear so that when the motor rotates the drive cables also move.

• The guides are fixed to the glass panel so that the panel is moved by the drive cables sliding the guides.

1 | Glass panel
2 | Sunroof motor
3 | Drive cable
4 | Frame
5 | Fully closed
6 | Guide
7 | Tilt up
8 | Fully open