#
CLUTCH MASTER CYLINDER DISASSEMBLY/ASSEMBLY

BHE051041990W02

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

L.H.D.

1 | Hose clip
2 | Reserve tank hose
3 | Joint
4 | Bushing
5 | Bolt
6 | Packing
7 | Connector
8 | Packing
9 | Snap ring (See Snap Ring Disassembly/Assembly Note.)
10 | Piston, secondary cup component
11 | Spacer
12 | Primary cup
13 | Return spring
14 | Clutch master cylinder body

R.H.D.

1 | Hose clip
2 | Reserve tank hose
3 | Joint
4 | Bushing
5 | Snap ring (See Snap Ring Disassembly/Assembly Note.)
6 | Piston, secondary cup component
7 | Spacer
8 | Primary cup
9 | Return spring
10 | Clutch master cylinder body

## Snap Ring Disassembly/Assembly Note

1. While pressing the piston in with a cloth-wrapped pin punch to protect the push rod contacting surface, remove/install the snap ring.